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PRISMATIC FITTING
ITEM NO: VT-8020; WATTS: 20W 
  [image: ]                      
    
	Item No:
	VT-8020

	SKU Code
	[bookmark: _GoBack]4991:4500K

	Real Watts
	20W

	EQ. Watts
	100W

	Voltage
	AC:200~240V

	Input Frequency
	50Hz

	Input Efficiency
	80lm/w

	Lumen(lm)
	1600lm

	PF
	>0.9

	CRI
	>80

	Color Temperature
	3000K,4500K,6000K

	Beam Angle
	110’D

	LED Chip
	SMD

	Protection Class
	IP20

	Body Material
	Aluminum+Plastic

	Dimmable
	No

	Unit size
	L:600x75x25mm

	Life Time
	20000hrs

	Operation Temperature
	-25 ~50’C

	Applicable Environment
	[bookmark: OLE_LINK3][bookmark: OLE_LINK4]Indoor Lighting, Used in Home down light, Stairwell lighting.
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